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Appendix B 
Sample Schematic Diagram 
 
The following schematic diagram is for the function: 
F(A,B,X,Y)=AXY’+ABY’+B’X’Y+A’X’Y+A’B’Y+BXY’ 
 
[image: Logic circuit diagram illustrating a combinational logic design using switches SW1 to SW4 as inputs labeled X, Y, A, and B, connected through logic gates (AND, OR, NOT) and integrated circuits (7404, 7411, 7432) to control output LED1 (F). The diagram includes labeled ICs and gate connections, showing signal flow from inputs through multiple AND and OR gates to produce a final output, highlighting the use of standard TTL logic components.] 
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